{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Datasheet","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":40,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Datasheet","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[[0,1,0,7],[1,1,1,7],[2,1,2,7],[3,1,3,7],[4,1,4,7]]}
["Directions:","wedges 1 and 2 do not need to be equal and opposite"]
[null,"prime denotes slope with respect to normal voltage"]
[null,"R/h can be estimated with manufacturer reports "]
[null,"Input AFM data into gray cells "]
[null,"Use the solver function (data tab; add-in) to iterate output variables until residual is minimized"]
[]
[null,null,"inputs",null,null,null,null,"outputs"]
[]
[null,"angle (°)","D'","W'","R/h",null,"µ","S","O/h"]
["wedge 1",5,5,5,0,null,7.1208842623612947E-2,{"$f":"((G10/D10)+(G11/D11))/2","v":1.4241795691788992E-2},1.6178862372474255E-2]
["wedge 2",5,5,5,null,null,7.1209114294276982E-2]
[]
[]
[]
[null,"Eq. 11",{"$f":"1/D10*(G10/(COS(B10*PI()/180)^2-G10^2*SIN(B10*PI()/180)^2)*(1-E10*(1-COS(B10*PI()/180))))","v":1.4351335823785222E-2},null,null,null,{"$f":"ROUND(G10,3)","v":7.0999999999999994E-2},{"$f":"ROUND(H10,3)","v":1.4E-2},{"$f":"ROUND(I10,3)","v":1.6E-2}]
[null,"Eq. 12",{"$f":"1/D11*(G11/(COS(B11*PI()/180)^2-G11^2*SIN(B11*PI()/180)^2)*(1-E10*(1-COS(B11*PI()/180))))","v":1.4351390580181337E-2},null,null,null,{"$f":"ROUND(G11,3)","v":7.0999999999999994E-2}]
[null,"Eq. 13",{"$f":"1/C10*((G10^2+1)*SIN(B10*PI()/180)*COS(B10*PI()/180)/(COS(B10*PI()/180)^2-G10^2*SIN(B10*PI()/180)^2)*(1-E10*(1-COS(B10*PI()/180)))-I10-E10*SIN(B10*PI()/180))","v":1.435136857170582E-2},null,null,null,{"$f":"ROUND(C20,3)","v":0}]
[null,"Eq. 14",{"$f":"1/C11*((G11^2+1)*SIN(B11*PI()/180)*COS(B11*PI()/180)/(COS(B11*PI()/180)^2-G11^2*SIN(B11*PI()/180)^2)*(1-E10*(1-COS(B11*PI()/180)))-I10-E10*SIN(B11*PI()/180))","v":1.4351369253941666E-2}]
[]
[null,"residual",{"$f":"STDEV(C15:C18)","v":2.2597771862361002E-8}]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}